

Record of emergency plumbing work in remote Aboriginal communities

Part 4A of the Plumbers Licensing and Plumbing Standards Regulations 2000

**Service provider:**       **Community:**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| **Date work completed** | **Category of work** | **Address** | **Authorised worker** | **Notes** |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |
|  |  |  |  |  |

**Category of work**

|  |  |
| --- | --- |
| (a) | replacing leaking tap washers, spindles, handles and shower roses (except when additional plumbing work is required) |
| (b) | replacing “P-Traps” and “S-Traps” in readily accessible locations, such as under sinks, basins or troughs |
| (c) | replacing leaking hose taps and hose tap vacuum breakers |
| (d) | replacing leaking cistern inlet and outlet washers and valves |
| (e) | capping a burst water main, damaged waste pipe or sanitary drain for the purposes of preventing a risk to human health or safety or a significant waste of water |
| (f) | replacing general covers (e.g. missing or broken inspection mounds, gully mounds, grates and vent cowls) |
| (g) | clearing blocked waste pipes and drains by the use of plungers, flexible hand rods or hand-held water hoses only |
| (h) | unblocking toilets, showers, basins, troughs, sinks and baths by the use of plungers, flexible hand rods or hand-held water hoses only |